|  |  |  |
| --- | --- | --- |
| **1** | **Product name** | **Ellipse Raised Bed** |
| **2** | **Short brief** | Add a touch of elegance and functionality to your outdoor space with our rectangular gabion raised garden bed planter. This versatile planter is perfect for growing a variety of plants, including flowers, vegetables, herbs, and shrubs. It can also be used to create a unique and eye-catching focal point in your garden or patio.. |
| **3** | **Product 3D view** |  |
| **4** | **Overview** | The rectangular gabion raised garden bed planter is made of high-quality galvanized steel wire mesh, which is rust-resistant and weatherproof. This ensures that your planter will last for many years to come, even in the harshest weather conditions.The rectangular gabion raised garden bed planter is also very sturdy and durable, thanks to its sturdy construction and transverse and longitudinal wires welded at every intersection. This means that it can support a variety of plants and soil, without the risk of collapsing or warping.In addition to its durability and functionality, the rectangular gabion raised garden bed planter is also incredibly easy to assemble and maintain. Simply fill it with rocks, gravel, or other decorative materials to create a secure and stylish border for your garden bed.

|  |  |  |
| --- | --- | --- |
| Article Number  | Outer Dimensions  | Inner dimensions  |
| GR1210 | 1500x500x500 | 1200x300x500 |
| GR1220 | 4000x500x500 | 3800x300x500 |
| GR1230 | 2000x1000x500 | 1800x800x500 |
| GR1240 | 3000x1000x1000 | 2800x800x1000 |
| GR1250 | 4000x1000x1000 | 3800x800x1000 |
| GR1260 | 6000x1000x1000 | 5800x800x1000 |

 |
| **5** | **Features**  | * Multiple variants are available
* Wire diameter of 4 mm
* Mesh size 100x50mm
* Adds visual interest to your garden or patio
* Rust and corrosion resistant
* Better Life
* Galvanized
* High Load Capacity (1400 kg/m3)
* Easy to assemble and maintain
* Versatile design can be used for a variety of purposes
* Custom finish coating available
* Multiple colors are available
* Stylish design
* 100% Tested
 |
| **6** | **Technical Specifications** |

|  |  |
| --- | --- |
| Material  | Carbon steel wire  |
| Wire Diameter | 4.00mm |
| Wall Thickness  | 100mm |
| Mesh Size  | 100x50 mm |
| Spiral coil wire diameter  | 3mm  |
| Spiral coil inner diameter  | 20 mm  |
| Spiral Pitch  | 45mm  |
| Load Capacity  | 1400 kg/m3 |
| Assembly Required  | Yes  |
| Rust proof  | Yes  |
| Finishing  | Galvanized/ PVC coating  |
| Color | Silver  |

 |
| **7** | **Application** | * Parks
* School
* Hotels
* Public Building
* Offices
* Outdoor spaces
* Residential
* Demarcation
* Sports Center
 |
| **8** | **Finishes** | * Products are hot deep Galvanized to BS EN 1461 or Equivalent standards.
* Galvanized and Powder coated to BS EN 13438 or Equivalent standards.
* Only powder coating to non-standard
* Marine coat Coating for application near salt water
 |
| **9** | **STANDARD COLOURS** | * Galvanized
* PVC Ral black 9005
* Custom colors and coating are available
 |
| **10** | **Installation** | At Hitech Gabion, we provide premium gabion products tailored to your needs and offer comprehensive support for your project's success. While we don't directly offer installation services, our expert team is available to provide detailed instruction manuals and consultancy to guide you through the installation process. If you require additional installation support, we can connect you with trusted construction vendors. Your satisfaction and project success are our top priorities, and we're committed to helping you achieve outstanding results every step of the way. |
| **11** | **Downloads** | 1. **Installation manual**
2. **Product data sheet**
3. **Drawing PDF**
4. **Tech specification MS word**
 |
| **12** | **Approvals** |  |